{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","Sheet2"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":34,"n_cols":20,"rows_kept":34,"cut":false,"hidden":false,"merged":[[18,15,18,16],[13,6,13,8],[13,9,13,11],[13,12,13,14],[13,15,13,16],[14,6,14,8],[14,9,14,11],[14,12,14,14],[14,15,14,16],[15,6,15,9],[15,10,15,13],[15,14,15,16],[16,6,16,9],[16,10,16,13],[16,14,16,16],[1,17,2,19],[0,0,0,19],[21,1,21,2],[10,10,10,13],[10,14,10,16],[7,0,8,0],[12,3,12,5],[13,3,13,5],[19,0,24,0],[19,1,20,2],[21,3,21,5],[7,5,7,8],[7,9,7,12],[9,3,9,5],[9,6,9,9],[10,3,10,5],[10,6,10,9],[11,3,11,5],[17,6,17,8],[17,9,17,11],[17,12,17,14],[17,15,17,16],[18,6,18,8],[18,9,18,11],[30,1,32,1],[29,1,29,2],[29,3,29,5],[29,6,29,8],[29,9,29,11],[29,12,29,14],[29,15,29,16],[30,3,30,5],[30,6,30,8],[30,9,30,11],[30,12,30,14],[31,6,31,8],[31,9,31,11],[31,15,31,16],[32,3,32,5],[32,6,32,8],[26,1,26,5],[26,6,26,11],[26,12,26,16],[27,3,28,10],[27,11,28,16],[22,3,22,5],[22,6,22,9],[22,10,22,13],[22,14,22,16],[23,3,23,5],[24,3,24,5],[24,6,24,9],[24,10,24,13],[24,14,24,16],[3,0,6,0],[14,3,14,5],[21,10,21,13],[5,1,6,2],[9,1,10,2],[11,1,12,2],[13,1,14,2],[15,1,16,2],[17,1,18,2],[7,1,7,4],[8,1,8,4],[21,6,21,9],[19,3,19,16],[20,3,20,16],[6,11,6,12],[9,10,9,13],[9,14,9,16],[11,6,11,9],[11,10,11,13],[11,14,11,16],[12,6,12,9],[12,10,12,13],[12,14,12,16],[18,12,18,14],[33,12,35,19],[33,0,35,11],[9,0,18,0],[21,14,21,16],[15,3,15,5],[17,3,17,5],[18,3,18,5],[16,3,16,5],[23,6,23,9],[23,10,23,13],[23,14,23,16],[32,9,32,11],[32,12,32,14],[32,15,32,16],[31,12,31,14],[27,0,32,0],[27,1,28,2],[22,1,24,1],[30,15,30,16],[31,3,31,5],[25,0,26,0],[25,1,25,5],[25,12,25,16],[25,6,25,11],[1,14,1,16],[2,5,2,7],[2,8,2,10],[2,11,2,13],[2,14,2,16],[1,0,2,0],[1,5,1,7],[1,8,1,10],[1,11,1,13],[1,1,1,4],[2,1,2,4],[3,3,3,4],[3,5,3,6],[5,3,5,4],[5,5,5,6],[4,3,4,4],[4,5,4,6],[6,3,6,4],[4,7,4,8],[3,1,4,2],[5,7,5,8],[6,7,6,8],[6,5,6,6],[4,15,4,16],[3,7,3,8],[3,9,3,10],[3,11,3,12],[3,13,3,14],[3,15,3,16],[7,13,7,16],[8,5,8,8],[8,9,8,12],[8,13,8,16],[5,9,5,10],[6,9,6,10],[5,15,5,16],[6,15,6,16],[5,13,5,14],[6,13,6,14],[5,11,5,12],[4,9,4,10],[4,11,4,12],[4,13,4,14]]}
["MAX77650"]
["Global\nResources","Software Reset",null,null,null,"nEN Pin Debounce Timer",null,null,"nEN Input Default Configuration",null,null,"Main Bias Enable Controller",null,null,"Main Bias Low Power Mode",null,null,"Output"]
[null,"No Action",null,null,null,"100us",null,null,"Push-Button Mode",null,null,"On/Off Controller",null,null,"Disabled"]
["Interruput\nMask/Unmask","Global\nInterruputs",null,"GPI Falling",null,"GPI Rising",null,"nEN Falling",null,"nEN Rising",null,"Thermal Alarm 1",null,"Thermal Alarm 2",null,"LDO Dropout ",null,"Register Name","Address","Data"]
[null,null,null,"Mask",null,"Mask",null,"Mask",null,"Mask",null,"Mask",null,"Mask",null,"Mask",null,"INTM_GLBL","0x06","0xFF"]
[null,"Charger\nInterruputs",null,"Thermistor",null,"Charger",null,"CHGIN",null,"Die Junction Temperture",null,"CHGIN Control",null,"VSYS Control",null,"VSYS Configuration Error",null,"INT_M_CHG","0x07","0xFF"]
[null,null,null,"Mask",null,"Mask",null,"Mask",null,"Mask",null,"Mask",null,"Mask",null,"Mask",null,"CNFG_GLBL","0x10","0x00"]
["GPIO","GPIO Direction",null,null,null,"GPO Driver Type",null,null,null,"GPO Data Output Value",null,null,null,"GPI Debounce Timer",null,null,null,"CNFG_GPIO","0x12","0x01"]
[null,"Input",null,null,null,"Open-Drain",null,null,null,"Logic Low",null,null,null,"0 ms(No Debounce)",null,null,null,"CNFG_CHG_A","0x18","0x00"]
["Charger","Step1",null,"Charger Enable",null,null,"Prequal Charger Current",null,null,null,"Battery Prequal Voltage Threshold",null,null,null,"Fast-Charge Safety Timer",null,null,"CNFG_CHG_B","0x19","0x00"]
[null,null,null,"Disable",null,null,0.1,null,null,null,"3.0V",null,null,null,"3 hours",null,null,"CNFG_CHG_C","0x1A","0xF8"]
[null,"Step2",null,"Fast-Charge Current(7.5mA-300.0mA)",null,null,"Fast-Charge Voltage(3.6V-4.6V)",null,null,null,"JEITA-Modified IFAST_CHG(7.5mA-300.0mA)",null,null,null,"VFAST_CHG JEITA(3.6V-4.6V)",null,null,"CNFG_CHG_D","0x1B","0x10"]
[null,null,null,15,null,null,3.6,null,null,null,15,null,null,null,3.6,null,null,"CNFG_CHG_E","0x1C","0x05"]
[null,"Step3",null,"Termination Current Threshold",null,null,"Top-Off Timer Length",null,null,"ICHGIN Limit",null,null,"Minimum VCHGIN",null,null,"VSYS Regulation(4.100V-4.800V)",null,"CNFG_CHG_F","0x1D","0x04"]
[null,null,null,"15.0% of IFAST_CHG",null,null,"0min",null,null,"0x0=95mA(ICHGIN_LIM_DEF=0)|475mA(ICHGIN_LIM_DEF=1)",null,null,"4.0V",null,null,4.5,null,"CNFG_CHG_G","0x1E","0x00"]
[null,"Step4",null,"Die Junction Temperature Point",null,null,"USB Suspend Mode",null,null,null,"Discharge Current Full Scale",null,null,null,"AMUX Selection",null,null,"CNFG_CHG_H","0x1F","0x00"]
[null,null,null,"60¡ãC",null,null,"CHGIN Not Suspended",null,null,null,"300.0mA",null,null,null,"OFF",null,null,"CNFG_CHG_I","0x20","0xF0"]
[null,"Step5",null,"Thermistor",null,null,"JEITA T1(Cold)",null,null,"JEITA T2(Cool)",null,null,"JEITA T3(Warm)",null,null,"JEITA T4(Hot)",null,"CNFG_SBB_TOP","0x28","0x01"]
[null,null,null,"Disable",null,null,"0.867V(5°C for β = 3380K)",null,null,"0.747V(15°C for β = 3380K)",null,null,"0.511V(35°C for β = 3380K)",null,null,"0.411V(45°C for β = 3380K)",null,"CNFG_SBB0_A","0x29","0xF2"]
["SIMO \nBuck-Boost","TOP Configuration",null,"Drive Strength Trim",null,null,null,null,null,null,null,null,null,null,null,null,null,"CNFG_SBB0_B","0x2A","0x08"]
[null,null,null,"0x1=Slower Than 0x0",null,null,null,null,null,null,null,null,null,null,null,null,null,"CNFG_SBB1_A","0x2B","0xE0"]
[null,null,null,"Target Output Voltage1",null,null,"Peak Current Limit",null,null,null,"Enable Control",null,null,null,"Active-Discharge",null,null,"CNFG_SBB1_B","0x2C","0x0B"]
[null,"Channel","SBB0",2.0499999999999998,null,null,"0.500A",null,null,null,"FPS Slot 0",null,null,null,"Enable",null,null,"CNFG_SBB2_A","0x2D","0xF2"]
[null,null,"SBB1",1.2,null,null,"0.500A",null,null,null,"FPS Slot 3",null,null,null,"Enable",null,null,"CNFG_SBB2_B","0x2E","0x08"]
[null,null,"SBB2",3.3,null,null,"0.500A",null,null,null,"FPS Slot 0",null,null,null,"Enable",null,null,"CNFG_LDO_A","0x38","0x28"]
["LDO","Target Output Voltage(1.3500V-2.9375V)",null,null,null,null,"Enable Control",null,null,null,null,null,"Active-Discharge",null,null,null,null,"CNFG_LDO_B","0x39","0x09"]
[null,1.85,null,null,null,null,"FPS Slot 1",null,null,null,null,null,"Enable",null,null,null,null,"CNFG_LED0_A","0x40","0x04"]
["LED Driver","TOP Configuration",null,"Master LED Driver Enable",null,null,null,null,null,null,null,"Enable",null,null,null,null,null,"CNFG_LED1_A","0x41","0x04"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"CNFG_LED2_A","0x42","0x04"]
[null,null,null,"Brightness(0%-100%)",null,null,"Invert",null,null,"Full Scale Current",null,null,"Duty Cycle",null,null,"Period",null,"CNFG_LED0_B","0x43","0x0F"]
[null,"Channel","LED0",0.15625,null,null,"In-Phase Operation",null,null,"Disabled",null,null,1,null,null,"0.5s",null,"CNFG_LED1_B","0x44","0x0F"]
[null,null,"LED1",0.15625,null,null,"In-Phase Operation",null,null,"Disabled",null,null,1,null,null,"0.5s",null,"CNFG_LED2_B","0x45","0x0F"]
[null,null,"LED2",0.15625,null,null,"In-Phase Operation",null,null,"Disabled",null,null,1,null,null,"0.5s",null,"CNFG_LED_TOP","0x46","0x0D"]
["Notes:1.Target Output Voltage:SBB0: From 0.800V to 2.375V. SBB1: From 0.8000V to 1.5875V. SBB2: From 0.80V to 3.75V.  \n               The letters will turn red if the input is out of range.\n             2.The values to be entered in the table can only be entered as numeric values, no units need to be entered.\n             3.The file named 'MAX77650 Configuration.txt' will be generated under the current directory.If the file already exists, it will be overwritten."]

{"sheet":"Sheet2","index":1,"n_rows":32,"n_cols":2,"rows_kept":32,"cut":false,"hidden":true,"merged":[]}
[null,"ICHGIN"]
[null,"95mA(ICHGIN_LIM_DEF=0)|475mA(ICHGIN_LIM_DEF=1)"]
[null,"190mA(ICHGIN_LIM_DEF=0)|475mA(ICHGIN_LIM_DEF=1)"]
[null,"285mA(ICHGIN_LIM_DEF=0)|475mA(ICHGIN_LIM_DEF=1)"]
[null,"380mA(ICHGIN_LIM_DEF=0)|475mA(ICHGIN_LIM_DEF=1)"]
[null,"475mA(ICHGIN_LIM_DEF=0)|95mA(ICHGIN_LIM_DEF=1)"]
[]
[]
[]
[null,"JEITA T1 (Cold)"]
[null,"1.024V(-10°C for β = 3380K)"]
[null,"0.976V(-5°C for β = 3380K)"]
[null,"0.923V(0°C for β = 3380K)"]
[null,"0.867V(5°C for β = 3380K)"]
[]
[null,"JEITA T2 (Cool)"]
[null,"0.923V(0°C for β = 3380K)"]
[null,"0.867V(5°C for β = 3380K)"]
[null,"0.807V(10°C for β = 3380K)"]
[null,"0.747V(15°C for β = 3380K)"]
[]
[null,"JEITA T3 (Warm)"]
[null,"0.511V(35°C for β = 3380K)"]
[null,"0.459V(40°C for β = 3380K)"]
[null,"0.411V(45°C for β = 3380K)"]
[null,"0.367V(50°C for β = 3380K)"]
[]
[null,"JEITA T4 (Hot)"]
[null,"0.411V(45°C for β = 3380K)"]
[null,"0.367V(50°C for β = 3380K)"]
[null,"0.327V(55°C for β = 3380K)"]
[null,"0.291V(60°C for β = 3380K)"]