{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","Sheet2"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":27,"n_cols":16,"rows_kept":27,"cut":false,"hidden":false,"merged":[[26,0,28,15],[25,1,25,3],[24,2,24,3],[23,4,25,5],[23,6,25,13],[21,0,25,0],[21,2,21,3],[22,2,22,3],[23,2,23,3],[21,4,22,5],[21,6,22,7],[21,8,22,9],[21,10,22,11],[21,12,22,13],[19,12,19,13],[20,12,20,13],[8,12,8,13],[9,12,9,13],[11,12,11,13],[9,10,9,11],[8,4,8,5],[19,10,19,11],[20,10,20,11],[15,12,15,13],[14,12,14,13],[13,12,13,13],[12,12,12,13],[10,12,10,13],[17,12,17,13],[18,10,18,11],[18,12,18,13],[16,12,16,13],[14,10,14,11],[15,10,15,11],[17,10,17,11],[10,10,10,11],[11,10,11,11],[12,10,12,11],[19,0,20,0],[9,2,9,3],[10,2,10,3],[19,2,19,3],[20,2,20,3],[20,6,20,7],[19,6,19,7],[20,4,20,5],[19,8,19,9],[20,8,20,9],[10,0,11,0],[18,8,18,9],[13,8,13,9],[14,8,14,9],[15,8,15,9],[19,4,19,5],[17,0,18,0],[17,2,17,3],[18,2,18,3],[17,4,17,5],[18,4,18,5],[17,8,17,9],[17,6,17,7],[18,6,18,7],[12,0,16,0],[0,0,0,15],[9,6,9,7],[10,6,10,7],[11,6,11,7],[12,6,12,7],[13,6,13,7],[14,6,14,7],[15,6,15,7],[16,6,16,7],[9,8,9,9],[10,8,10,9],[11,8,11,9],[12,8,12,9],[9,4,9,5],[10,4,10,5],[11,4,11,5],[12,4,12,5],[13,4,13,5],[8,0,9,0],[7,0,7,1],[5,0,6,1],[1,14,1,15],[8,6,8,7],[16,2,16,3],[11,2,11,3],[12,2,12,3],[13,2,13,3],[14,2,14,3],[15,2,15,3],[8,2,8,3],[7,12,7,13],[14,4,14,5],[15,4,15,5],[8,8,8,9],[8,10,8,11],[16,8,16,9],[16,4,16,5],[13,10,13,11],[16,10,16,11],[1,0,2,1],[1,10,1,13],[2,10,2,13],[3,0,4,1],[5,2,5,5],[5,6,5,9],[5,10,5,13],[7,2,7,3],[7,4,7,5],[7,6,7,7],[7,8,7,9],[7,10,7,11],[1,2,1,5],[1,6,1,9],[2,2,2,5],[2,6,2,9],[3,2,3,7],[3,8,3,13],[4,2,4,7],[4,8,4,13],[6,2,6,5],[6,6,6,9],[6,10,6,13]]}
["MAX31790"]
["Global Configuration",null,"Bus Timeout",null,null,null,"Oscillator Selection",null,null,null,"I²C Watchdog",null,null,null,"Output"]
[null,null,"Disable",null,null,null,"Internal",null,null,null,"Inactive",null,null,null,"Address","Data"]
["PWM Frequency",null,"PWM1-3 Frequency",null,null,null,null,null,"PWM4-6 Frequency",null,null,null,null,null,"00h","  "]
[null,null,"25kHz",null,null,null,null,null,"25kHz",null,null,null,null,null,"01h","  "]
["Failed Fan Options",null,"Sequential Start Delay",null,null,null,"Failed Fan Option",null,null,null,"Fault Queue",null,null,null,"02h","  "]
[null,null,"500ms",null,null,null,"Continue Operation",null,null,null,"2 Faults",null,null,null,"03h","  "]
[null,null,"Fan Channel 1",null,"Fan Channel 2",null,"Fan Channel 3",null,"Fan Channel 4",null,"Fan Channel 5",null,"Fan Channel 6",null,"04h","  "]
["Mode","PWMOUT Act As","PWM",null,"PWM",null,"PWM",null,"PWM",null,"TACH11",null,"TACH12",null,"05h","  "]
[null,"Mode","PWM",null,"RPM",null,"RPM",null,"PWM",null,"PWM",null,"RPM",null,"06h","  "]
["PWM\n Setting","Rate of Change","15.6ms",null,"15.6ms",null,"1.9ms",null,"1.9ms",null,"1.9ms",null,"15.6ms",null,"07h","  "]
[null,"Asymmetric Rate of Change","Disable",null,"Disable",null,"Disable",null,"Disable",null,"Disable",null,"Disable",null,"08h","  "]
["Tachometer\nSetting","Speed Range",1,null,1,null,4,null,4,null,16,null,16,null,"09h","  "]
[null,"Control/Monitor","Control",null,"Control",null,"Control",null,"Control",null,"Monitor Only",null,"Monitor Only",null,"0Ah","  "]
[null,"TACH Input","Enable",null,"Enable",null,"Enable",null,"Enable",null,"Enable",null,"Enable",null,"0Bh","  "]
[null,"TACH/Locked Rotor","TACH",null,"TACH",null,"TACH",null,"TACH",null,"TACH",null,"Locked Rotor",null,"0Ch","  "]
[null,"Locked Rotor Polarity","High",null,"High",null,"High",null,"High",null,"High",null,"Low",null,"0Dh","  "]
["Options","Spin-Up","2 TACH counts or 1s",null,"2 TACH counts or 1s",null,"2 TACH counts or 2s",null,"2 TACH counts or 1s",null,"2 TACH counts or 0.5s",null,"No Spin-Up",null,"12h","  "]
[null,"Window (0-255)",0,null,0,null,0,null,0,null,0,null,0,null,"13h","  "]
["Fan Faults\nMask","Fan 1-6 Mask","Disable",null,"Disable",null,"Enable",null,"Enable",null,"Enable",null,"Enable",null,"14h","  "]
[null,"Fan 7-12 Mask","Disable",null,"Disable",null,"Enable",null,"Enable",null,"Enable",null,"Disable",null,"60h","  "]
["Calculator","Actual RPM",0,null,null,null,null,null,null,null,null,null,null,null,"61h","  "]
[null,"NP*",2,null,null,null,null,null,null,null,null,null,null,null,"62h","  "]
[null,"SR*",4,null,null,null,null,null,null,null,null,null,null,null,"63h","  "]
[null,"TACH Count (Hex)","0000h",null,null,null,null,null,null,null,null,null,null,null,"64h","  "]
[null,"TACH Count = (60/(NP*RPM))*SR*8192",null,null,null,null,null,null,null,null,null,null,null,null,"65h","  "]
["Notes: 1. NP = Number of tachometer pulses per revolution.  Most general-purpose brushless DC fans produce two tachometer pulses per revolution. \n               2. SR = 1, 2, 4, 8, 16, or 32. This is the number of tachometer periods over which the tachometer clock is counted.\n               3. About the Speed Range setting, please refer to datasheet page 27 for more detail.\n               4. If the absolute difference between TACH Counter and TACH Target count is less than the value in the Window Register.  The update rate of the PWM duty cycle is slowed to 1LSB per second.\n               5. The file named 'MAX31790.txt' will be generated under the current directory.  If the file already exists, it will be overwritten."]

{"sheet":"Sheet2","index":1,"n_rows":5,"n_cols":7,"rows_kept":5,"cut":false,"hidden":true,"merged":[]}
[null,"Input","Input2","Input3","Input4","Enable5","Enable6"]
["Enable","Enable","Enable","Enable","Enable","Enable","Enable"]
["Disable"]
[null,"Enable","Enable","Enable","Enable","Enable","Enable"]
[null,"Disable","Disable","Disable","Disable","Disable","Disable"]