{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Sheet1","Sheet2"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":26,"n_cols":13,"rows_kept":26,"cut":false,"hidden":false,"merged":[[1,10,24,10],[23,1,23,2],[24,1,24,2],[1,0,1,2],[22,1,22,2],[9,0,12,0],[13,0,15,0],[22,0,24,0],[16,0,21,0],[10,1,10,2],[23,6,24,9],[19,7,19,8],[20,7,20,8],[21,7,21,8],[22,7,22,8],[12,1,12,2],[9,1,9,4],[13,1,13,4],[14,1,14,2],[21,1,21,2],[19,1,19,2],[11,1,11,2],[18,1,18,2],[17,1,17,2],[20,1,20,2],[16,1,16,4],[6,1,6,4],[3,1,3,2],[4,1,4,2],[5,1,5,2],[7,1,7,2],[14,8,14,9],[7,7,7,8],[9,7,9,8],[11,7,11,8],[16,6,18,9],[8,7,8,8],[14,6,14,7],[12,6,13,6],[12,9,13,9],[12,7,13,8],[15,6,15,7],[15,8,15,9],[25,0,30,12],[8,1,8,2],[15,1,15,2],[1,11,1,12],[0,0,0,12],[10,7,10,8],[2,0,5,0],[6,0,8,0],[2,1,2,4],[2,7,2,8],[3,7,3,8],[4,6,4,9],[1,6,1,9],[5,7,5,8],[6,7,6,8],[1,5,24,5]]}
["MAX6639"]
["Fan Controls",null,null,"Fan 1","Fan 2",null,"Global Configuration",null,null,null,null,"Output"]
["Step1","Fan Information",null,null,null,null,"SMBus Timeout","Temp Channel 2 Source",null,"PWM High Frequency",null,"Address","Data"]
[null,"Fan Select",null,"3-wire fan","3-wire fan",null,"Enable","Local",null,"Disable",null,"03h","  "]
[null,"RPM Range Select",null,"16000RPM","8000RPM",null,"Mask & Temperature",null,null,null,null,"04h","  "]
[null,"Pulses per Revolution",null,2,2,null,null,"Channel 1",null,"Channel 2",null,"08h","  "]
["Step2","Control Mode",null,null,null,null,"ALERT Mask","Disable",null,"Disable",null,"09h","  "]
[null,"Control Mode",null,"Automatic RPM Control","PWM Control",null,"ALERT Temperature Limit(°C) ",85,null,85,null,"0Ah","  "]
[null,"Channel Control",null,"None","None",null,"OT Mask","Disable",null,"Disable",null,"0Bh","  "]
["Step3","PWM Setting",null,null,null,null,"OT Limit(°C) ",110,null,110,null,"0Ch","  "]
[null,"Frequency",null,"33.33Hz","33.33Hz",null,"THERM Mask","Disable",null,"Enable",null,"0Dh","  "]
[null,"Polarity",null,"Positive","Positive",null,"THERM Temperature Limit(°C) ",85,null,85,null,"10h","  "]
[null,"Rate of Change",null,"0.0625s","0s",null,"Minimum\nFan Start Temperature(°C) ",40,null,40,null,"11h","  "]
["Step4","Tachometer Setting",null,null,null,null,null,null,null,null,null,"12h","  "]
[null,"Start Tachometer Count(Hex)",null,"FF","FF",null,"Fan 1 Fault Mask",null,"Fan 2 Fault Mask",null,null,"13h","  "]
[null,"Min Tachometer Count(Hex)*",null,0,0,null,"Enable",null,"Enable",null,null,"14h","  "]
["Step5","RPM Setting",null,null,null,null,null,null,null,null,null,"15h","  "]
[null,"RPM step-size A",null,3,6,null,null,null,null,null,null,"16h","  "]
[null,"Temp step-size",null,"2°C","4°C",null,null,null,null,null,null,"17h","  "]
[null,"RPM step-size B",null,16,10,null,null,"Fan 1",null,"Fan 2",null,"22h","  "]
[null,"Start step-size B*",null,3,7,null,"Actual RPM",0,null,0,null,"23h","  "]
[null,"Min. Speed",null,"0% Duty Cycle","0% Duty Cycle",null,"Actual Fan Pulses Per Revolution",2,null,2,null,"24h","  "]
["Options","Fan Spin Up",null,"Enable","Enable",null,"Tachometer Count Value","00h",null,"00h",null,"25h","  "]
[null,"THERM to Fan Full Speed",null,"Disable","Disable",null," Tachometer count value = (((internal clock frequency) x 60) / actual RPM)* （selected number of pulses per revolution / actual fan pulses)",null,null,null,null,"28h","  "]
[null,"Pulse Stretching",null,"Enable","Enable",null,null,null,null,null,null,"29h","  "]
["Notes: According to the maximum fan speed used in application to set RPM Range Select:\n              1. Min Tachometer Count (Hex):  This sets the minimum allowable fan tachometer count (maximum speed).  It limits the maximum speed of the fan to reduce noise at high temperatures. \n              2. Start step-size B: Select the number of temperature/tachometer steps above the fan-start temperature at which step-size B begins. \n              3. If Automatic RPM Control is selected, the fan will start to spin up to the defined speed in the Start Tachometer.   When the temperature reaches Minimum Fan Start Temperature the temperature \n                   changes.\n             4. Temp step-size: The fan speed will change by RPM step-size A, if the steps number changed in step-size A is larger than the value of Start step-size B.  If the steps number is changed, the fan speed \n                  will change by RPM step-size B value.\n             5. The file named 'MAX6639.txt' will be generated under the current directory.  If the file already exists, it will be overwritten."]

{"sheet":"Sheet2","index":1,"n_rows":17,"n_cols":9,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
[null,"PWM","RPM"]
[null,"0s",null,null,null,"Enable","Disable","20Hz","5kHz"]
[null,"0.0625s","0.0625s","0.0625s",null,"Disable",null,"33.33Hz","8.33kHz"]
[null,"0.125s","0.125s","0.125s",null,null,null,"50Hz","12.5kHz"]
[null,"0.25s","0.25s","0.25s",null,null,null,"100Hz","25kHz"]
[null,"0.5s","0.5s","0.5s"]
[null,"1s","1s","1s"]
[null,"2s","2s","2s"]
[null,"4s","4s","4s"]
[null,"Automatic_RPM_Control"]
[null,"PWM_Control"]
[]
[]
["None","None","None",null,null,"Enable","Disable","Enable","Disable"]
["RPM",null,"Channel 1",null,null,"Disable",null,"Disable"]
["PWM",null,"Channel 2",null,null,"wfan3",null,"nfan3"]
[null,null,"Both"]