{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":29,"n_cols":4,"rows_kept":29,"cut":false,"hidden":false,"merged":[[25,1,25,4],[26,1,26,4],[27,1,27,4],[28,1,28,4],[20,0,20,4],[21,1,21,4],[22,1,22,4],[23,1,23,4],[24,1,24,4],[17,3,17,4],[18,3,18,4],[0,0,0,4],[1,0,3,4],[19,0,19,4],[13,1,15,1],[13,2,14,3],[15,2,15,3],[4,0,4,4],[5,0,18,0],[5,4,15,4]]}
[" Reserve Power Calculator  "]
["Welcome to the Maxim Integrated Reserve Power Calculator. To calculate:\n     1. Enter your values in the green boxes.\n     2. Click \"Check Values\" to ensure they are valid.  \n     3. If there are no comments in the \"Errors and Notes\" column, click \"Calculate\" to \n         get your final value. \nIf you are still having trouble with number assignments, please refer to the Number Entry Guide below."]
[]
[]
[]
[null,null,"Your Values","Errors and Notes"]
[null,"VCAP MAX (V)",2.65," "]
[null,"VCAP MIN (V)",1.55," "]
[null,"tBU (s)",9.48," "]
[null,"VSYS (V)",4," "]
[null,"VSYS  (V)",3.04," "]
[null,"ISYS_LOAD (A)",0.2," "]
[null,"Efficiency η (%)",92," "]
[]
[]
[null,null,"Note: Check values and correct errors before calculating."]
[]
[null,"ELOAD (J)",5.763840000000001,"Energy supplied to the system load during backup"]
[null,"Supercap (F)",2.7121400338791655,"Perhaps round to nearest standard value"]
[]
["Number Entry Guide"]
["Input","Explanation"]
["VCAP MAX (V)","2.7V maximum super capacitor rating, 4.5V device maximum; must be below 90% of VSYS,100mV resolution "]
["VCAP MIN (V)","0.8V to VCAP max range,100mV resolution"]
["tBU (s)\nBack UpTime","1ms to 10s range"]
["VSYS (V)","2.5V to 5.0V range,100mV resolution"]
["VSYS (V)","Boost phase target voltage, 80% duty cycle limitation during boosting,100mV resolution"]
["ISYS_LOAD (A)","Calculations are based on following values with 5% regulation:\n1.  Inductor value= 1uH( As per EVK)  \n2. Ton time= 320 ns (Minimum value as per datasheet)\n3. Ipeak current = 2A (Minimum value as per datasheet)\nIsys_load value will vary based on efficiency. Please refer to TOC#9 in datasheet. "]
["Efficiency\n η (%)","Please refer to TOC#9 in datasheet to deternimine efficiency value  for \ncorrosponding output volatge and load current"]